{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet2","index":0,"n_rows":46,"n_cols":6,"rows_kept":46,"merged":[[0,0,0,5],[2,0,6,0],[7,0,11,0],[12,0,24,0],[16,5,17,5],[23,5,24,5],[25,0,33,0],[27,5,28,5],[34,5,36,5],[36,0,40,0],[37,3,37,4],[38,3,38,4],[41,0,44,0],[45,0,45,1],[45,2,45,5]],"flags":["formulas_cached_only"]}
["省级/区  域级土壤中心实验室设备配套方案"]
["产品类别","产品名称","推荐型号","市场价","规格，备注","仪器用途"]
["样品采集设备","土壤有机物采样器","JC-803C",6500,"采样管直径38mm，长241mm，采样长度20cm。标准配置采样深度2m。","用于土壤有机物分析采样"]
[null,"活塞式柱状采泥器","JC-801A",6800,"不锈钢切割头（常规分析采样），工程塑料切割头（重金属分析采样）","用于采集底泥，常规分析、重金属分析"]
[null,"土壤重金属采样器","JC-803D",6000,"采样直径5cm、一次采样长度20cm，一次单点采样量1kg左右","用于土壤重金属分析采样"]
[null,"土壤采样器","JC-803B",7000,"标配土壤钻头：沙土钻头、粘土钻头、多石钻头、泥浆土钻头、螺旋钻头，","土壤常规分析采样"]
[null,"无扰动采样器","JC-WGR01",1000,"一个采样套筒+20个采样管","土壤挥发性性有机物采样配套气象色谱使用"]
["风干设备","电热鼓风干燥箱","101系列-3B",6800,"内尺寸60*50*75cm。","用于实验室配件清洗后的干燥，消毒"]
[null,"土壤干燥箱","JC-TR-24",26000,"24位","土壤样品干燥，风干，温度恒定。避免样品二次损坏"]
[null,"样品冷藏箱","YC-100",4500,"澳柯玛。100L","用于对有机样品的冷藏（冻）保存"]
[null,"冷冻干燥机","JC-LDZG-10S",22000,"台式","对于有机样品测试样品以冷冻方式进行干燥不破坏样品性质，去除样品水分"]
[null,"除湿机","JC-CS26L",2500,"26L","用于室内除湿，保持室内空气干燥"]
["样品前处理设备","筛分机","JC-SF",3500,"主机+6层筛子","用于筛选不同粒径的样品"]
[null,"行星式球磨机","JC-QM-1",30000,"1L主机+四套250ml玛瑙罐","用于研磨土壤样品，粉碎土壤粒径，满足实验要求"]
[null,"微波消解仪","JC-600W",78000,"6位，含赶酸","用于土壤重金属消解"]
[null,"全自动土壤样品制备系统","JC-FASP","198w","标配","用于土壤样品全自动，标准化制备"]
[null,"索氏提取仪","JC-ST-06",6000,"6位，土壤专用","用于土壤有机物的提取"]
[null,"快速溶剂提取","BASE-26","35W","标配"]
[null,"固相萃取仪","JC-GX-24S",4500,"圆形，24位","用于土壤中的多环芳羟及有机氯等污染物的前处理"]
[null,"氮吹仪","JC-WD-24",4800,"圆形水浴.24位","用于有机物的快速浓缩"]
[null,"电炉","DL-1",400,"单联","样品加热消化"]
[null,"水浴锅","HH系列-6",1000,"双列6孔","样品加热消化"]
[null,"土壤有机碳恒温加热器","JC-YJT-12",6000,"主机+12根消解管","用于土壤有机碳测量的前处理"]
[null,"混匀仪","JC-XW-D",2000,"多用头","用于对样品的混匀，保证样品均匀性一致"]
[null,"混匀仪（多功能振荡器）","JC-GGC6000",3000,"回旋，多用"]
["元素分析设备","便携式土壤重金属X射线荧光光谱仪","JC-HMI(II)",210000,"34项目","用于土壤重金属现场分析和初步检测"]
[null,"电感耦合等离子体发射光谱仪","JC-ICP-01",300000,"标配","用于分析周期表中所有金属元素和部分非金属元素"]
[null,"原子吸收分光光度计","JC-YZ-100",90000,"火焰性，三灯座","用于Cd、Cu、Pb、Zn等重金属的测定，根绝元素不同选择不同的规格和仪器"]
[null,"原子吸收分光光度计","JC-YZ-100",160000,"火焰石墨一体机"]
[null,"原子荧光分光光度计","JC-YG-200",118000,"任选两灯，可选配自动进样器","用于As、Cd、Hg等元素的测定"]
[null,"测汞仪","F732系列-VJ",12800,"冷原子吸收法","用于Hg元素的测定"]
[null,"分光光度计","JC-UT2000",12800,"带软件","用于稀土总量的测定"]
[null,"气相色谱仪","JC-7890",98000,"主机+ECD检测器+毛细管进样器+色谱工作站+弄残专用柱+氮气钢瓶+电脑打印机","土壤质量六六六和滴滴涕、有机氯农药测定"]
[null,"气相色谱-质谱联用仪","JC-6800",320000,"标配","土壤和沉积物、二噁英类和挥发性有机物检测"]
[null,"各类天平","FA2204B",3200,"万分之一，220g,其他量程可选","用于各个环节的样品称量"]
[null,"各类天平","JA5003N",3000,"千分之一，300g,其他量程可选"]
["其他配套设备","各类天平","YP10002",1600,"百分之一，量程1000g,其他量程可选"]
[null,"样品存放架","根据具体需求推荐","需提供实验室需要的尺寸进行定制",null," "]
[null,"实验操作台","根据需求定制","需提供实验室需要的尺寸进行定制",null,"用于样品制备，存放等各个环节的操作使用"]
[null,"超声波清洗器","JC-QX-30L",4800,"30L,其他尺寸可选","用于实验室配件的清洗"]
[null,"全自动洗瓶机","JC-XPJ-200",128000,"200L的其他尺寸可选","用于实验室玻璃器皿的全自动清洗"]
["现场检测设备","便携式土壤墒情检测仪","JC-TR-4G",12000,"PH,盐分，水分，温度","用于检测土壤温度、水分、盐分、PH等原位测量"]
[null,"便携式土壤养分检测仪","JC-TY04",20000,"主机+配件箱+土壤氮磷钾试剂","用于检测土壤中氮磷钾、有机质、中微量元素等快速现场检测"]
[null,"便携式氧化还原电位仪","TR-901",7600,"标配","用于现场原位测试新鮮鲜或湿润土壤的氧化还原电位，符合《HJ746-2015土壤氧化还原电位的测定电位法》标准。"]
[null,"便携式紧实度测量仪","JC-JSD01",8000,"标配","紧实的土壤可阻止水分的入渗，降低化肥的利用率，影响植物根系生长，甚至导致作物减产"]
["备注",null,"1.本报价含13%发票，含包装费，含运输费\n2.付款方式：100%预付，款到发货\n3.交货时间：以合同签订要求为准 "]

{"sheet":"Sheet3","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}