{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":53,"n_cols":4,"rows_kept":53,"merged":[[0,0,0,3],[2,0,5,0],[6,0,7,0],[10,0,12,0],[13,0,14,0],[20,0,21,0],[23,0,25,0],[28,0,29,0],[28,1,29,1],[28,3,29,3],[33,0,34,0],[36,0,48,0],[49,0,51,0],[52,1,52,3]],"flags":["formulas_cached_only"]}
["疾控中心仪器设备配套方案"]
["检测项目","产品名称","规格","常用型号"]
["微生物","美国3MATP荧光检测仪","标配","LM1"]
[null,"微生物气溶胶浓缩器","含液体式冲击式采样器","KW-1"]
[null,"六级筛孔撞击式微生物采样器","28.3L/min","FA-1"]
[null,"菌落计数器","标配","XK97-A"]
["相对湿度","机械通风干湿表","10%RH～100%RH","DHM2"]
[null,"电动通风干湿表","10%RH～100%RH/ -36℃～46℃","HM3"]
["温湿度","温湿度计","标配","TES-1360A"]
["风速仪","热线式风速仪","0.1 ~ 30.0 m/s","TES-1340"]
["压力","数字式微压计","标配","DP1000-IIIB"]
[null,"标准皮托管","30mm","L型皮托管"]
[null,"空盒气压表","平原式/ 800～1060hpa","DYM3"]
["噪声","多功能声级计","2级、统计、存储、含AH40打印机，","AWA5688"]
[null,"声级校准器","2级校准器","AWA6022A"]
["旋光度","阿贝折射仪","1.30000--1.70000(nD)","JCZ-600"]
["照度","照度计","20/200/2000/20000 Lux","TES-1330A"]
["辐射热","辐射热计","0～10KW/㎡","MR-5"]
["黑球，湿球温度","热指数仪","黑球温度范围5～120℃/±0.5℃","WBGT-2006"]
["辐射","紫外辐照计","λ：(275～330)nm；λp=297nm","UV-B"]
["电磁场强度","工频近区电场强度测量仪","30 Hz～2000Hz","RJ-5"]
[null,"高频近区电磁场强度测量仪","200kHz－30MHz","RJ-2"]
["粉尘","中流量颗粒物采样器","Pm10/pm2.5","JCH-120F"]
["大气","双路恒流大气采样器","甲醛/苯/二甲苯","JCH-2400"]
[null,"大气采样器","0.1-1.2L/min","QC-2B"]
[null,"大流量大气采样器","0.1-5L/min","QC-5"]
["氡","测氡仪","空气氡+土壤氡","FD216"]
["酸碱度","PH计","标配","PHB-4"]
["浊度","便携式浊度测试仪","0～20NU","JC-WGZ-200B"]
[null,null,"0～200NTU"]
["呼吸性粉尘","多功能粉尘仪","Pm2.5/pm10","JCF-5C"]
["红外一氧化碳","非色散红外一氧化碳","0-50PPM","JC-3011A"]
["红外二氧化碳","非色散红外二氧化碳","0-10000PPM","JC-3010E(S)"]
["流量校准","皂膜流量计","校5-5000ml/min","JCL-2010(S)"]
[null,"皂膜流量计","校1-1000ml/min","JC-2010(s)"]
["粒度分析","粒度分析仪","0～150µm","MD-1"]
["实验室设备","分光光度计","610nm",721]
[null,"高压灭菌锅","24L","24L"]
[null,"水浴锅","6孔","HH系列-6"]
[null,"千分之一天平","500g/1mg","JC5003CH"]
[null,"涡旋混合器","标配","JC-XW-I"]
[null,"涡旋振荡器","回旋","JC-GGC-12H"]
[null,"电热恒温培养箱","45*55*55/5-60度","HN系列-50BS"]
[null,"C02培养箱","80L","JC-CHP-80S"]
[null,"生物显微镜","双目","XSP-2CA"]
[null,"离心机","20ml","TDL-4"]
[null,"均质器","含50个均质袋","JC-JZ-08"]
[null,"干热灭菌箱","50L","JC-ARMJ-05A"]
[null,"新风量检测仪","含皮托管","TSI 9565A"]
["配套采样器使用的吸收瓶","U型多孔玻板吸收瓶","白色","25ml"]
[null,"大泡式吸收瓶","白色","10ml"]
[null,"冲击式吸收瓶","白色","15ml"]
["备注","1.本报价含13%发票，含包装费，含运输费\n2.付款方式：100%预付，款到发货\n3.交货时间：以合同签订要求为准"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}