{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet3","index":0,"n_rows":16,"n_cols":4,"rows_kept":16,"merged":[[0,0,0,3],[15,1,15,3]],"flags":["formulas_cached_only"]}
["微生物检测—实验室常用"]
["序号","名称","常用型号","功能介绍"]
[1,"生物安全柜","BSC-1004/1304","为操作原代培养物、菌毒株以及诊断性标本等具有感染性的实验材料时，用来保护操作者本人、实验室环境以及实验材料"]
[2,"双人单面垂直送风净化工作台","SW-CJ-2D","准闭合式玻璃风门，可有效防止外部气流透入，及操作异味对人体的刺激"]
[3,"电热恒温培养箱","HN系列","水体分析和BOD测定细菌、霉菌、微生物的培养、保存、植物栽培、育种试验的专用恒温设备"]
[4,"低温生化培养箱","JC-DRH-80/160/250","培养血清、药品、微生物培养环境试验的专用低温设备"]
[5,"电热鼓风恒温干燥箱","101系列","用于物品的烘焙，干燥，热处理和热加工、农业生产，科学研究，医疗卫生单位，实验实均可使用"]
[6,"高压灭菌锅","8L/18L/24L","采用电加热水，在密闭的条件下，产生饱和蒸汽，对灭菌对象迅速潮润、加热、渗透，经一段时间的保压保温。使微生物被杀灭，达到灭菌目的"]
[7,"双目显微镜","XSP系列-2CA","应用了光学原理的显微放大技术，对采集的细微样品制作成标本，进行显微技术的放大和观察"]
[8,"万分之一电子分析天平（内校）","FA1004C","性能更加稳定，且反应速度更快，同时具有积分可调和稳定度、灵敏度可调功能"]
[9,"便携式PH计|酸度计|酸度检测仪","PHB-4","实验室精密测量溶液pH值和电极电位"]
[10,"实用型实验室专用纯水机","JC-ROS-10/ 20","采用预处理、反渗透技术、超纯化处理以及后级处理等方法，将水中的导电介质去除"]
[11,"恒温水浴锅","HH-6","水浴恒温加热和其它温度试验"]
[12,"六级筛孔撞击式空气微生物采样器","FA-1","双功能阶式多级撞击采样器"]
[13,"全自动旋转振荡器","JC-GGC1000","实验室样品前处理"]
["备注","1.本报价含13%发票，含包装费，含运输费\n2.付款方式：100%预付，款到发货\n3.交货时间：以合同签订要求为准 "]