{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet3","index":0,"n_rows":23,"n_cols":4,"rows_kept":23,"merged":[[0,0,0,3],[22,1,22,3]],"flags":["formulas_cached_only"]}
["化妆品业—实验室常用"]
["序号","名称","常用型号","功能介绍"]
[1,"全自动微量水分测定仪","JC-SF-1","适用于大部分液体、气体、固体物质中水分的测定"]
[2,"扫描型紫外可见分光光度计","UV759","高分辨率，地杂散光，液晶屏显示的紫外可见分光光度计"]
[3,"傅立叶变换红外光谱仪","FSM1201型","测量各种气体、固体、液体样品的吸收、反射光谱等，而且可用于短时间化学反应测量"]
[4,"气相色谱仪","JC-2011","定性、定量分析"]
[5,"氮氢空一体机发生器","JC-XDT-300","氢气、氮气、空气发生器"]
[6,"梯度液相色谱仪","LC600B","定性、定量分析"]
[7,"超声波清洗器","JC-QX","除其本身具有的清洗功能外，还具有提取、乳化、加速溶解、粉碎、分散等多种功能"]
[8,"全自动旋转振荡器","JC-GGC1000","实验室样品前处理"]
[9,"低温生化培养箱","JC-DRH-80/160/250","培养血清、药品、微生物培养环境试验的专用低温设备"]
[10,"电热鼓风恒温干燥箱","101系列","用于物品的烘焙，干燥，热处理和热加工、农业生产，科学研究，医疗卫生单位，实验实均可使用"]
[11,"便携式PH计|酸度计|酸度检测仪","PHB-4","实验室精密测量溶液pH值和电极电位"]
[12,"粘度计","VM4000","测量流体粘度的高精度测试仪器"]
[13,"显微热台熔点仪","JCR-350","测量结晶性化学制品、药品和部分结晶聚合物熔点"]
[14,"邵氏硬度计","TIME5410","测量硬度"]
[15,"全自动折光仪","JCZ-200","高效、高精确测量透明、半透明、深色、粘稠状等各类液体的折射率(nD)和糖溶液的质量分数"]
[16,"立式真空干燥箱","JC-DZS-6060/6080/6210","适合于对干燥热敏性、易氧化物质和复杂成分物品进行快速的干燥处理"]
[17,"高压灭菌锅","8L/18L/24L","采用电加热水，在密闭的条件下，产生饱和蒸汽，对灭菌对象迅速潮润、加热、渗透，经一段时间的保压保温。使微生物被杀灭，达灭菌目的"]
[18,"旋涡混合器","JC-XW-II","用于血常规末稍血液的混匀且不破坏血细胞"]
[19,"重金属快速检测定仪","JC-12C","重金属检测仪可快速检测食品中的金属铅、砷、铬、镉、汞等金属"]
[20,"恒温水浴锅","HH-6","水浴恒温加热和其它温度试验"]
["备注","1.本报价含13%发票，含包装费，含运输费\n2.付款方式：100%预付，款到发货\n3.交货时间：以合同签订要求为准 "]