{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet3","index":0,"n_rows":22,"n_cols":5,"rows_kept":22,"merged":[[0,0,0,4],[21,0,21,4]],"flags":["formulas_cached_only"]}
["酒厂实验室---采购指南"]
["检测项目","产品名称","产品型号","规格","符合标准"]
["测量水质浊度","浊度仪","JC-BZ-1T","0-1000NTU"]
["测透明半透明液体或固体的折射率和平均色散","阿贝折射仪","JCZ-600","1.30000--1.70000(nD)","各类液体的折射率"]
["测产品颜色","色差计","NS800","45°/0°(45°环形均匀照明0°","CIE No.15，GB/T 3978."]
["测电解质溶液电导率值","电导率仪","DDBJ-350",null,"便携式电导率"]
["定量分析","分光光度计",722,"波长范围：320-1020nm"]
["测产品含水量","卡尔费休水份测定仪","JC-SF-3","测量范围：3μg~100mgH2O（3ppm~100%含水量）"]
["测量物质对不同波长单色辐射的吸收程度，定量分析","紫外可见分光光度计","UV759CRT","190-1100nm"]
["测物质旋光度，分析物质的浓度、纯度、含糖量","自动旋光仪","JCX-P610","旋光度、比旋度、浓度、糖度"]
["测定钠离子浓度","钠离子浓度计","JC-NaS-50","0-1000mg/L"]
["定性定量分析","气相色谱仪","JC-7890","室温5℃-400℃"]
["测PH值","酸度计","PHB-4","0-14","便携式现场用"]
["测定溶液中的糖度、含糖量","手持糖量计","PAL-1","0.0 至53.0%糖度0.1%"]
["测溶解氧","溶解氧测定仪","JPBJ-608","(0.00～19.99)mg/L"]
["观察微小物质","显微镜","XSP-2CA","双目"]
["根据被测元素的基本原子对特征辐射的吸收程度进行定量分析","原子吸收分光光度计","JC-YZ-600","自动型火焰石墨炉一体机（8灯座）"]
["定性定量分析","液相色谱仪","LC600B","流量设定范围：0.001～9.999mL/min（以0.001mL/min步长调节流量）"]
["测量非透明材料表面颜色","比较测色仪","WSL-2"]
["测啤酒浊度","啤酒浊度检测仪","JC-XZ-1A-Z","0-200NTU、0-50EBC"]
["测产品颜色","色度计","NS800","45°/0°(45°环形均匀照明0°","CIE No.15，GB/T 3978."]
["1.本报价含13%发票，含包装费，含运输费\n2.付款方式：100%预付，款到发货\n3.交货时间：以合同签订要求为准 "]