{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":21,"n_cols":6,"rows_kept":21,"merged":[[0,0,0,5],[20,0,20,1],[20,2,20,5]],"flags":["formulas_cached_only"]}
["实验室基础设备配套方案"]
["序号","名称","规格","单位","数量","作用"]
[1,"普通电子精密天平","1000g/10mg","台",2,"样品称量"]
[2,"千分之一电子分析天平","300g/1mg","台",2,"样品称量"]
[3,"万分之一电子分析天平","220g/0.1mg","台",2,"样品称量"]
[4,"十万分之一电子分析天平","52g/0.01mg","台",2,"样品称量（推荐进口，此型号品牌为梅特勒托利多）"]
[]
[5,"高压灭菌锅","18L","台",1,"玻璃器皿的杀菌"]
[6,"超声波清洗器","30L","台",2,"玻璃器皿及器材的清洗"]
[7,"台式低速离心机","4000转/分","台",1,"分离液体与固体颗粒或液体与液体的混合物"]
[8,"超纯水机","20L/H","台",1,"制备纯水/超纯水"]
[9,"紫外可见分光光度计","波长范围","台",1,"对物质进行定量或定性的分析"]
[10,"测汞仪","汞的测量","台",1,"汞的测量"]
[11,"原子吸收分光光度计","石墨火焰一体机","台",1,"主要用于微量元素和痕量分析测量及分析"]
[12,"原子荧光分光光度计","三灯三通道","台",1,"样品中砷、汞、硒、锡、铅、铋、锑、碲、锗、镉、锌等十一种元素的痕量分析测量。"]
[13,"离子色谱仪","标配","台",1,"对样品中的阳离子，阴离子进行分析和测量"]
[14,"气相色谱仪","配置定制","台",1,"根据测的项目不同，进行配置"]
[15,"恒温恒湿培养箱","150L","台",1,"细菌及细胞培养"]
[16,"电热鼓风干燥箱","220L","台",1,"排除标本内的残留水分、微生物用玻璃器皿的干热杀菌、加热实验之前的预热"]
[17,"电加热板","标配","台",3,"样品加热"]
["备注",null,"1.本报价含13%发票，含包装费，含运输费\n2.付款方式：100%预付，款到发货\n3.交货时间：以合同签订要求为准 "]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}